**FELT ACOUSTIC UNDERLAY SPECIFICATIONS**

Color –Black

Roll size- 39.37” \* 366.14” (100 SQ.ft.roll)

Thickness – 3mm

(+/ - 5% Manufacturing Tolerance)

Impact Sound Transmission

Class (IIC) = 69

ASTM – E492 – 90 (ASTM – E989 – 89)

Class (STC) = 70

Acoustic Transmission Loss

ASTM – E90 – 02 (ASTM – E413 -87)